**Steps to configure the wireless router for the EDT network**

1. Unlock the wireless router enclosure
2. Insert the EDT SIM card
3. Lock the wireless router enclosure
4. Unplug the wireless router from the power source and plug it in again - so that it re-initializes
5. On the EDT computer open Internet Explorer
6. Type in the address bar: <http://192.168.1.1>
7. Select Admin and enter admin as password
8. Once logged in go to Advanced Settings|Dial-up Settings|Profile Settings
   1. Enter EDT under profile name (profile list)
   2. Clear the username and password fields
   3. Under the APN replace what is there with nmpc.com.na
   4. Save or Apply changes
9. Click on Advanced Settings|Dial-up Settings|PPP Settings
   1. In the window that appears verify that the connection is on Auto
   2. Select Authentication mode: CHAP+PAP
   3. Select EDT under the Profile list
   4. Save changes - Apply
10. Click on Security|Virtual Server
    1. Under Name enter FTP
    2. Enter the IP Address as 192.168.1.100
    3. Select FTP(21) from common ports
    4. Set the Status to On
    5. Click on OK, and then on Apply, Edit
    6. After the verification process is over Enter RDP under Name
    7. Enter the IP Address as 192.168.1.100
    8. Set the Status to On
    9. Set WAN and LAN Port to 3389
    10. Click on OK, and then on Apply
11. Test remote desktop connection using the EDT SIM card’s IP address