**\*\*\* STEPS TO GO TO THE EDT MOBILE MAIN MENU \*\*\***

1. REMOVE BATTERY (wait for at least 10 seconds before replacing it, to allow the device to reset)
2. IF YOU SEE SYSTEM ERROR MESSAGE POWER OF DEVICE AND START FROM STEP 1 ABOVE
3. DRV TO FORMAT: KEY IN **1** and **ENT** to FORMAT **DRIVE "A"**
4. SYSTEM MENU – KEY IN **1** to **EXECUTE AP** and **ENT** to **CONFIRM**
5. EDT MAIN MENU: 1. DISPENSE

!9. SETUP – DATE/TIME

9. SETUP – 4. LOAD FILES.....

(SWITCH OFF USB CRADLE AND ON AGAIN IF ERROR RECEIVED)

**\*\*\* STEPS TO INSTALL THE NEW USB-BLUETOOTH CRADLE TO WORK WITH THE EDT MOBILE \*\*\***

1. C:\Program Files (x86)\CASIO\LMWIN\lmwin.ini (NOTEPAD++)- set MINIMIZE=OFF (SAVE)
2. TASK SCHEDULE – CREATE EDT BACKUP – COPY TO BEFORE FOLDER/EXTERNAL DRIVE
3. INSTALL UPDATED EDT [JUNE 2014] (RUN X 2) - START MENU (RESTORE EDT) - OPEN EDT ON DESKTOP - SUPERUSER - ADMIN-SETUP-GLF- LINE 44 - Validation= n 0. – USER MENU – EXPORT/IMPORT DATA- CREATE FILES - LINK (STEP NO 2).
4. DOWNLOAD/UPLOAD UTILITY – STOP LM – CONFIGURE – SELECT “IOBOX” – START LM.

**ONLY USE THE STEPS BELOW IF YOU WANT TO OVERRIDE ALL DATA ON THE EDT MOBILE WITH GUIDANCE FROM IT SUPPORT**

**\*\*\* STEPS TO COPY ONE EDT MOBILE SOFTWARE TO THE OTHER EDT MOBILE \*\*\***

1. ALL STEPS BELOW SHOULD BE PERFORMED TO BOTH DEVICES, UNLESS IF OTHERWISE SPECIFIED
2. REMOVE BATTERY DEVICE (wait for about 10 seconds before replacing it back)
3. KEY 1 and ENT to FORMAT DRIVE "A"
4. SET THE CORRECT DATE/TIME:
   1. SYSTEM MENU – 3. DATE/TIME
   2. KEY ENT and CLR to go to SYSTEM MENU
5. DUPLICATE DEVICE SOFTWARE:
   1. SYSTEM MENU - 4.TRANSMIT - 3. DUPLICATE HT - 3. Drive - 3. A + B Drive
   2. **ENT** and **CLR** to go back to DUPLICATE HT MENU
   3. **FROM** DEVICE Only: 1. SEND -SEND-
   4. **TO** DEVICE Only: 2. RECEIVE -RECEIVE-
   5. ENSURE THAT THE BASES OF BOTH DEVICES FACE EACH OTHER AND WAIT FOR THE DUPLICATE PROCESS TO COMPLETE (you will see the main dispensing menu on the “to device”)
6. ON THE FROM DEVICE KEY CLR UNTIL YOU GET TO THE SYSTEM MENU
   1. KEY IN **1** to **EXECUTE AP** and **ENT** to **CONFIRM** (you will see the main dispensing menu)

**\*\*\* STEPS TO MANUALLY FORMAT DRIVE B \*\*\***

1. SYSTEM MENU - 4.TRANSMIT - 4. UTILITY - 2. FORMAT DRIVE 2. B DRIVE